
===============================================================================
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
				                      Help File
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
===============================================================================
Viewing Shadin Avionics ETM Recorder 943200-1X .etm files in FleetView:

1. Ensure FleetView is installed on the PC.
  - If FleetView is not installed there is a copy of FleetView 7.30 available 
    on this USB, for the latest version of FleetView visit www.Shadin.com

2. Install the USB drive with .etm files into any available USB port on the PC.

3. Run FV_import.exe (searches the USB ports for .etm files)

4. A dialog will prompt the user with the number of files found on the USB ports
   verify the number .etm files and click 'YES'

5. Select existing home base file directory from the list or create
   a new home base file directory by typing in the space, then click 'OK'

6. A dialog will prompt the user with the number of files converted and the 
   number of files that already exist in the home base file directory
   - If any faults are encountered during the conversion a dialog will prompt
     the user.  

7. Open FleetView program then click the 'Tools' drop down and select 'Convert'

8. Under 'Select File(s)' on the left side click the home base file directory 
   for the files you want to convert.  On the right side check the box next to 
   the files that need to be converted then click 'Done'

9. The FleetView conversion is complete and the reports can be viewed by 
   selecting the file under the home base file directory under 'Database' 

For technical support contact Shadin Avionics at 1-800-388-2849

===============================================================================
End of Help file
